{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":53,"n_cols":5,"rows_kept":53,"cut":false,"hidden":false,"merged":[[29,0,29,4],[33,0,33,4],[38,0,38,4],[50,0,50,4],[0,0,0,5],[1,0,1,3],[3,0,3,4],[12,0,12,4],[21,0,21,4],[24,0,24,4]]}
[" ARK | 比较 产品"]
["2019/10/21 10:00:04"]
[null,"Core™ i9-10940X","Core™ i9-10920X ","Core™ i9-10900X ","Core™ i9-10980XE Extreme"]
["基本要素"]
["产品集"," 酷睿™ X "," 酷睿™ X "," 酷睿™ X "," 酷睿™ X "]
["垂直市场","Desktop","Desktop","Desktop","Desktop"]
["处理器编号","i9-10940X","i9-10920X","i9-10900X","i9-10980XE"]
["状态","Launched","Launched","Launched","Launched"]
["发行日期","Q4'19","Q4'19","Q4'19","Q4'19"]
["光刻","14 nm","14 nm","14 nm","14 nm"]
["包括的项目","盒包无风扇","盒包无风扇","盒包无风扇","盒包无风扇"]
["建议客户价格","$797.00","$700.00","$599.00","$1000.00"]
["性能"]
["内核数","14","12","10","18"]
["线程数","28","24","20","36"]
["处理器基本频率","3.30 GHz","3.50 GHz","3.70 GHz","3.00 GHz"]
["最大睿频频率","4.60 GHz","4.60 GHz","4.50 GHz","4.60 GHz"]
["缓存","19.25 MB Smart Cache","19.25 MB Smart Cache","19.25 MB Smart Cache","24.75 MB Smart Cache"]
[" 睿频加速 Max 技术 3.0 频率 ‡","4.80 GHz","4.80 GHz","4.70 GHz","4.80 GHz"]
["TDP","165 W","165 W","165 W","165 W"]
["集成显卡","无","无","无","无"]
["补充信息"]
["提供嵌入式方案","否","否","否","否"]
["数据表","立即查看","立即查看","立即查看","立即查看"]
["内存规格"]
["最大内存大小（取决于内存类型）","256 GB","256 GB","256 GB","256 GB"]
["内存类型","DDR4-2933","DDR4-2933","DDR4-2933","DDR4-2933"]
["最大内存通道数","4","4","4","4"]
["ECC 内存支持 ‡","否","否","否","否"]
["扩展选项"]
["可扩展性","1S Only","1S Only","1S Only","1S Only"]
["PCI Express 修订版","3.0","3.0","3.0","3.0"]
["PCI Express 通道数的最大值","48","48","48","48"]
["封装规格"]
["支持的插槽","FCLGA2066","FCLGA2066","FCLGA2066","FCLGA2066"]
["最大 CPU 配置","1","1","1","1"]
["散热解决方案规范","PCG 2017X","PCG 2017X","PCG 2017X","PCG 2017X"]
["TJUNCTION","86°C","94°C","94°C","86°C"]
["先进技术"]
[" 深度学习提升","是","是","是","是"]
[" 傲腾™ 内存支持 ‡","是","是","是","是"]
[" 睿频加速 Max 技术 3.0 ‡","是","是","是","是"]
[" 睿频加速技术 ‡","2.0","2.0","2.0","2.0"]
[" 超线程技术 ‡","是","是","是","是"]
[" 虚拟化技术 ‡","是","是","是","是"]
[" 定向 I/O 虚拟化技术 ‡","是","是","是","是"]
[" 64 ‡","是","是","是","是"]
["指令集扩展","SSE4.1, SSE4.2, AVX2, AVX-512","SSE4.1, SSE4.2, AVX2, AVX-512","SSE4.1, SSE4.2, AVX2, AVX-512","SSE4.1, SSE4.2, AVX2, AVX-512"]
["AVX-512 FMA 单元数","2","2","2","2"]
["增强型英特尔 SpeedStep® 技术","是","是","是","是"]
["安全性与可靠性"]
[" AES 新指令：","是","是","是","是"]
["执行禁用位 ‡","是","是","是","是"]