{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":56,"n_cols":3,"rows_kept":56,"cut":false,"hidden":false,"merged":[[32,0,32,2],[36,0,36,2],[41,0,41,2],[53,0,53,2],[0,0,0,3],[1,0,1,3],[3,0,3,2],[12,0,12,2],[23,0,23,2],[27,0,27,2]]}
[" ARK | 比较英特尔® 产品"]
["2019/10/21 15:15:18"]
[null,"英特尔® 酷睿™ i7-7800X X 系列处理器","英特尔® 酷睿™ i7-7820X X 系列处理器"]
["基本要素"]
["产品集","英特尔® 酷睿™ X 系列处理器","英特尔® 酷睿™ X 系列处理器"]
["垂直市场","Desktop","Desktop"]
["处理器编号","i7-7800X","i7-7820X"]
["状态","Launched","Launched"]
["发行日期","Q2'17","Q2'17"]
["光刻","14 nm","14 nm"]
["包括的项目","Please note: The boxed product does not include a fan or heat sink","Please note: The boxed product does not include a fan or heat sink"]
["建议客户价格","$383.00 - $389.00","$589.00 - $599.00"]
["性能"]
["内核数","6","8"]
["线程数","12","16"]
["处理器基本频率","3.50 GHz","3.60 GHz"]
["最大睿频频率","4.00 GHz","4.30 GHz"]
["缓存","8.25 MB L3 Cache","11 MB L3 Cache"]
["总线速度","8 GT/s","8 GT/s"]
["QPI 链接数","0","0"]
["集成显卡","无","无"]
["TDP","140 W","140 W"]
["英特尔® 睿频加速 Max 技术 3.0 频率 ‡",null,"4.50 GHz"]
["补充信息"]
["提供嵌入式方案","否","否"]
["数据表","立即查看","立即查看"]
["产品简介","立即查看","立即查看"]
["内存规格"]
["最大内存大小（取决于内存类型）","128 GB","128 GB"]
["内存类型","DDR4-2400","DDR4-2666"]
["最大内存通道数","4","4"]
["ECC 内存支持 ‡","否","否"]
["扩展选项"]
["可扩展性","1S Only","1S Only"]
["PCI Express 修订版","3.0","3.0"]
["PCI Express 通道数的最大值","28","28"]
["封装规格"]
["支持的插槽","FCLGA2066","FCLGA2066"]
["最大 CPU 配置","1","1"]
["散热解决方案规范","PCG 2017X","PCG 2017X"]
["TJUNCTION","100°C","99°C"]
["先进技术"]
["英特尔® 傲腾™ 内存支持 ‡","是","是"]
["英特尔® 睿频加速技术 ‡","2.0","2.0"]
["英特尔® 超线程技术 ‡","是","是"]
["英特尔® 虚拟化技术 ‡","是","是"]
["英特尔® 定向 I/O 虚拟化技术 ‡","是","是"]
["英特尔® 64 ‡","是","是"]
["指令集","64-bit","64-bit"]
["指令集扩展","Intel® SSE4.1, Intel® SSE4.2, Intel® AVX2, Intel® AVX-512","Intel® SSE4.1, Intel® SSE4.2, Intel® AVX2, Intel® AVX-512"]
["AVX-512 FMA 单元数","2","2"]
["增强型英特尔 SpeedStep® 技术","是","是"]
["英特尔® 睿频加速 Max 技术 3.0 ‡",null,"是"]
["安全性与可靠性"]
["英特尔® AES 新指令：","是","是"]
["执行禁用位 ‡","是","是"]